#
TRANSMISSION/TRANSAXLE SPECIFICATIONS

id050000100600

## Clutch

Item | Specifications
--- | ---
Manual transaxle type | G35M-R | G66M-R | A26M-R | A26MX-R
Clutch control | Hydraulic
Clutch cover | Spring type | Diaphragm
Set load | (N {kgf, lbf}) | 5,200 {531, 1,169} | 6,000 {611, 1,350} | 10,100 {1,030, 2,271}
Clutch disc | Outer diameter | (mm {in}) | 215 {8.46} | 250 {9.84}
Inner diameter | (mm {in}) | 150 {5.91} | 150 {6.10}
Clutch pedal | Type | Suspended
Pedal ratio | 6.6
Full stroke | (mm {in}) | 140 {5.51}
Clutch master cylinder inner diameter | (mm {in}) | 15.87 {0.625}
Clutch release cylinder inner diameter | (mm {in}) | 19.05 {0.750}
Clutch fluid type | SAE J1703, FMVSS 116 DOT-3 or DOT-4

## Manual Transaxle [G35M-R]

Item | Specifications
--- | ---
Engine type |  | L8
Manual transaxle type |  | G35M-R
Operation system |  | Cable
Transaxle control |  | Floor-shift
Shift assist | Forward |  | Synchromesh
Reverse |  | Selective sliding and synchromesh
Gear ratio | 1GR |  | 3.666
2GR |  | 2.059
3GR |  | 1.392
4GR |  | 0.970
5GR |  | 0.755
Reverse |  | 3.166
Final gear ratio |  | 4.388
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10 °C {50 °F} | SAE 80W-90
Capacity (approx. quantity) | (L {US qt, Imp qt}) | 2.87 {3.03, 2.53}

## Manual Transaxle [G66M-R]

Item | Specifications
--- | ---
Engine type |  | LF | L3
Manual transaxle type |  | G66M-R
Operation system |  | Cable
Transaxle control |  | Floor-shift
Shift assist | Forward |  | Synchromesh
Reverse |
Gear ratio | 1GR |  | 3.454
2GR |  | 2.059 | 1.842
3GR |  | 1.310
4GR |  | 0.970 | 1.030
5GR |  | 0.795 | 0.837
6GR |  | 0.680 | 0.755
Reverse |  | 3.166
Final gear ratio |  | 4.388
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10 °C {50 °F} | SAE 80W-90
Capacity (approx. quantity) | (L {US qt, Imp qt}) | 2.95 {3.12, 2.60}

## Manual Transaxle [A26M-R, A26MX-R]

Item | Specifications
--- | ---
Engine type |  | MZR-CD (RF Turbo) | L3 Turbo
Manual transaxle type |  | A26M-R | A26MX-R
Operation system |  | Cable
Transaxle control |  | Floor-shift
Shift assist | Forward |  | Synchromesh
Reverse |  | Synchromesh (Lever type)
Gear ratio | 1GR |  | 3.538
2GR |  | 1.913 | 2.238
3GR |  | 1.218 | 1.535
4GR |  | 0.880 | 1.171
5GR |  | 0.809 | 1.085
6GR |  | 0.673 | 0.853
Reverse |  | 3.831
Final gear ratio | 1GR-4GR |  | 3.611 | 3.941
5GR, 6GR, Reverse |  | 3.095 | 3.350
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10 °C {50 °F} | SAE 75W-90
Capacity (approx. quantity) | (L {US qt, Imp qt}) | 2.55 {2.69, 2.24}

## Automatic Transaxle [FS5A-EL]

Item | Specification
--- | ---
Engine type | LF | L3
Automatic transaxle type | FS5A-EL
Gear ratio | 1GR | 3.620
2GR | 1.925
3GR | 1.285
4GR | 0.933
5GR | 0.692
Reverse | 3.405
Final gear ratio | 3.863
ATF | Type | ATF M-V
Capacity (Approx. quantity) | (L {US qt, lmp qt}) | 8.14 {8.60, 7.16}
Torque converter stall torque ratio | 2.07 | 1.84
Hydraulic system (Number of drive/driven gear plates) | Forward clutch | 4/4
3-4 clutch | 3/3
Reverse clutch | 2/2
Direct clutch | 2/3
Low and reverse brake | 5/5
Reduction brake | 3/5
Band servo | Servo diameter (Piston outer dia.) | (mm {in}) | 64.6 {2.54}
Front planetary gear (Number of teeth) | Front sun gear | 49
Front pinion gear | 20
Front internal gear | 89
Rear planetary gear (Number of teeth) | Rear sun gear | 37
Rear pinion gear | 30
Rear internal gear | 98
Primary gear (number of teeth) | 86
Secondary gear (number of teeth) | 82
Secondary planetary gear (Number of teeth) | Secondary sun gear | 31
Secondary pinion gear | 29
Secondary internal gear | 89
Output gear (number of teeth) | 22
Ring gear (number of teeth) | 85

## Automatic Transaxle [JA5AX-EL]

Item | Specification
--- | ---
Transaxle type | JA5AX-EL
Gear ratio | 1GR | 3.801
2GR | 2.131
3GR | 1.364
4GR | 0.935
5GR (O/D) | 0.685
Reverse | 2.970
Final gear ratio | 3.712
ATF | Type | ATF M-III or equivalent (e.g. Dexron®III)
Capacity (approximate quantity) (L {US qt, Imp qt}) | 8.3 {8.8, 7.3}
Torque converter stall torque ratio | 1.750:1
Hydraulic system (Number of drive/driven plates) | Low clutch | 6/6
2-4 brake | 3/2
High clutch | 5/5
Direct clutch | 3/5
Reverse clutch | 2/2
Low and reverse brake | 6/5
Band servo (mm {in}) | Reduction accumulator piston outer dia./reduction band servo piston outer dia. | 49.66/57.64
Number of front planetary gear teeth | Ring gear | 74
Sun gear | 34
Pinion gear | 20
Number of rear planetary gear teeth | Ring gear | 75
Sun gear | 42
Pinion gear | 17
Number of reduction planetary gear teeth | Ring gear | 85
Sun gear | 31
Pinion gear | 27
Number of output gear teeth | 41
Number of idler gear teeth | 47
Number of reduction gear teeth | 22
Number of ring gear teeth | 67

## Automatic Transaxle Shift Mechanism

Item | Specifications
--- | ---
Transaxle control | Floor-shift
Operation system | Cable