#
TCM REMOVAL/INSTALLATION [FS5A-EL]

id051721800400

1. Disconnect the negative battery cable.

2. For U. K. specs., perform the following procedures.

  (1) Remove the front side trim (left-side).
  (2) Partially peel back the flower covering.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

L.H.D..

.

1 | TCM connector
2 | TCM

R.H.D. (U.K. specs).

.

1 | Control unit bracket
2 | TCM connector
3 | TCM

R.H.D. (except U.K. specs).

.

1 | Control unit bracket
2 | TCM connector
3 | TCM

## Set Nut/bolt Removal Note

1. Using a chisel and hammer, cut a groove on the head of the set nut/bolt so that a screwdriver can be inserted.

2. Loose the set nut/bolt using an impact screwdriver or pliers.

## Set Nut/bolt Installation Note

1. Install a new set nut/bolt and tighten it until the neck of the nut/bolt is cut.