#
SUNROOF MOTOR REMOVAL

id091500800900

1. Disconnect the negative battery cable.

2. Turn the seaming welt and weatherstrip over.

3. Remove the sunroof seaming welt.

4. Remove the A-pillar trims.(See A-PILLAR TRIM REMOVAL.)

5. Remove the B-pillar upper trims.(See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

6. Remove the C-pillar trims.(See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].)(See C-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

7. Remove the D-pillar trims (WGN).(See D-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

8. Remove the front map light.(See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

9. Remove the rear map light.(See REAR MAP LIGHT REMOVAL/INSTALLATION.)

10. Remove the cargo compartment light (WGN).(See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN].)

11. Remove the sunvisors.(See (SUNVISOR REMOVAL/INSTALLATION.)

12. Remove the assist handle.(See ASSIST HANDLE REMOVAL/INSTALLATION.)

13. Remove the net anchor (WGN).

14. Remove the headliner.(See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].)(See HEADLINER REMOVAL/INSTALLATION [WGN].)

15. Disconnect the connector.

16. Remove the screws, and then remove the sunroof motor.