#
FOREWORD [JA5AX-EL]

id050206800200
• When the customer reports vehicle malfunction, check the malfunction indicator lamp (MIL) indication, AT warning indication, and diagnostic trouble code (DTC), then diagnose the malfunction according to following flowchart.

  - If the DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE [JA5AX-EL].)
  - If the DTC does not exist, the MIL and AT warning light does not illuminate, diagnose the applicable symptom troubleshooting. (See AUTOMATIC TRANSAXLE SYMPTOM TROUBLESHOOTING [JA5AX-EL].)

*:Malfunction Indicator lamp (MIL), AT warning light