#
BOOST SENSOR CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1740300
• Installed on the intake manifold with the bracket.

1 | Boost sensor
2 | Intake manifold

• When pressure is applied to the piezoelectric element in the sensor, an electric potential difference occurs. Output voltage increases as the intake air pressure increases.

.

1 | Boost sensor
2 | Boost sensor output voltage characteristic
3 | Intake air pressure
4 | Output voltage
5 | High
6 | Low