#
GENERATOR DISASSEMBLY/ASSEMBLY [L3 Turbo]

id0117b18004b2

  Caution

  • Melt the solder quickly, otherwise the diodes (rectifier) and regulator will be damaged by excessive heat.

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Front cover
2 | Pulley (See Pulley Disassembly/Assembly Note.)
3 | Rotor
4 | Bearing
5 | Generator heat insulator
6 | Stator coil
7 | Rectifier
8 | Brush holder
9 | Rear bracket

## Pulley Disassembly/Assembly Note

1. Disassemble/assemble the pulley using the SST.

Tightening torque

  60-85 N·m {6.1-8.7 kgf·m, 45-62 ft·lbf}