#
BUCKLE SWITCH INSPECTION

id081100803000

## Front Buckle

1. Disconnect the negative battery cable.

2. Disconnect the buckle switch connector.

3. Inspect for continuity between the buckle switch terminals using a tester.

  • If not as indicated in the table, replace the front buckle.

## Rear Buckle

### LH side, center

1. Disconnect the negative battery cable.

2. Disconnect the buckle switch connector.

3. Inspect for continuity between the buckle switch terminals using a tester.

  • If not as indicated in the table, replace the front buckle.

### RH side

1. Disconnect the negative battery cable.

2. Disconnect the buckle switch connector.

3. Inspect for continuity between the buckle switch terminals using a tester.

  • If not as indicated in the table, replace the front buckle.