AIR FUEL RATIO (A/F) SENSOR HEATER CONTROL OPERATION [MZR-CD (RF Turbo)]

id0140f1780300

Operation Conditions

• The PCM operates the A/F sensor heater when the following conditions are met.

Activation condition | Drive signal
--- | ---
• After the engine has started and a fixed period of time has elapsed (the elapsed time period after the engine starts is determined by exhaust gas temperature). • Battery positive voltage is 9 V or more and less than 16 V. | • The PCM outputs a duty signal. • The element temperature is measured by the impedance of the A/F sensor heater and a duty ratio is determined.