#
ELECTRONIC THROTTLE CONTROL OPERATION [L3 Turbo]

id0140b6100900
• Feedback control has been adopted to the throttle actuator and it is monitored by the TP sensor so that it reaches the target throttle opening angle.

## Target throttle opening angle

• Throttle opening angle according to the engine speed and target charging efficiency table has been set.

## Target charging efficiency table

• This table has been created by assuming a target charging efficiency according to the engine speed and virtual accelerator opening angle.

## Virtual accelerator opening angle

• The virtual accelerator opening angle has been set according to the gear position, vehicle speed, accelerator opening angle, and accelerator opening change rate to improve driveability.