AIR FUEL RATIO (A/F) SENSOR FUNCTION [MZR‐CD (RF Turbo)]

id0140f1256000

• The wide-range air/fuel ratio sensor, which can linearly detect the oxygen concentration (air/fuel ratio of the air-fuel mixture) in the exhaust gas in all ranges, from lean to rich, is used on the A/F sensor.
• A heater has been adopted on the A/F sensor, allowing stable detection of the oxygen concentration even when the exhaust gas temperature is low.
• The measured oxygen concentration is used for the exhaust gas recirculation (EGR) control.