#
DTC P0563 [MZR-CD (RF Turbo)]

id0102f1832700

DTC P0563 | Battery voltage high input
--- | ---
DETECTION CONDITION | • The PCM monitors the battery voltage. If the battery voltage is more than 16 V, the PCM determines that there is a malfunction in the battery charging system. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Generator malfunction • Battery malfunction • Connector or terminal malfunction • Short to power supply in wiring harness between generator terminal D and PCM terminal 9 • Related wiring harness malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT GENERATOR TERMINAL FOR POOR INSTALLATION • Turn the engine switch off. • Inspect generator terminal B for looseness. • Is there any malfunction? | Yes | Connect generator terminal B correctly, then go to Step 10.
No | Go to the next step.
5 | INSPECT GENERATOR • Inspect the generator. (See GENERATOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the generator, then go to Step 10. (See GENERATOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
6 | INSPECT BATTERY POSITIVE TERMINAL FOR POOR INSTALLATION • Turn the engine switch off. • Inspect the battery positive terminal for looseness. • Is there any malfunction? | Yes | Connect the battery positive terminal correctly, then go to Step 10.
No | Go to the next step.
7 | INSPECT BATTERY • Inspect the battery. (See BATTERY INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the battery, then go to Step 10. (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
8 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 6.
No | Go to the next step.
9 | INSPECT GENERATOR CIRCUIT SHORT CIRCUIT • Inspect for continuity between generator terminal D (wiring harness-side) and PCM terminal 9 • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for short, then go to the next step.
10 | VERIFY TROUBLESHOOTING OF DTC P0563 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
11 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.