#
NO.30 DOES NOT SHIFT DOWN IN M RANGE [JA5AX-EL]

id050305809200

30 | Does not shift up in M range
DESCRIPTION | • Gear position indicator light in instrument cluster illuminates, but vehicle does not downshift when selector is pushed lever to "-" side.
POSSIBLE CAUSE | • Down switch or related harness malfunction Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.