#
CAMSHAFT END PLAY INSPECTION [WITHOUT DIESEL PARTICULATE FILTER]

id0110f4501700

1. Install the camshaft cap and rocker arm shaft. (See Rocker Arm and Rocker Arm Shaft Assembly Note)

Standard end play

  0.03-0.16 mm {0.0012-0.0062 in}

Maximum end play

  0.20 mm {0.0079 in}

2. Measure the camshaft end play.

Replace the cylinder head or camshaft if necessary.

3. Remove the camshaft cap and rocker arm shaft. (See Rocker Arm and Rocker Arm Shaft Disassembly Note)