#
DTC B2229, B2231, B2233, B2235

id080200802200

DTC | B2229 | Passenger-side air bag module assembly incorrect
--- | --- | ---
B2231
B2233
B2235
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • If a SAS control module of different specification is assembled • If a different configuration setting has been performed • SAS control module internal malfunction
POSSIBLE CAUSE | • Passenger-side air bag module assembly incorrect • SAS control module assembly incorrect • SAS control module internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT SAS CONTROL MODULE • Verify that the correct SAS control module is assembled. | Yes | Go to the next step.
No | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
2 | INSPECT SAS CONTROL MODULE • Using the WDS or equivalent, perform SAS control module configuration. • Is DTC B2477 indicated? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.