#
FOREWORD [FS5A-EL]

id050221800200
• When the customer reports a vehicle malfunction, inspect the malfunction indicator lamp (MIL), AT warning light indication, and TCM memory for diagnostic trouble code (DTC), then diagnose the malfunction according to the following flowchart.

  - If a DTC exists, diagnose the applicable DTC. (See DTC TABLE [FS5A-EL].)
  - If no DTC exists, the MIL does not illuminate, and AT warning light does not illuminate. Diagnose the applicable symptom troubleshooting. (See SYMPTOM TROUBLESHOOTING ITEM TABLE [FS5A-EL].)

*: Malfunction indicator lamp (MIL), AT warning light