#
FRONT OIL SEAL REPLACEMENT [MZR-CD (RF Turbo)]

id0110f1800800

1. Remove the timing belt. (See TIMING BELT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove in the order shown in the table.

3. Install in the reverse order of removal.

1 | Timing belt pulley lock bolt (See Timing Belt Pulley Lock Bolt Removal/Installation Note)
2 | Timing belt pulley (See Timing Belt Pulley Removal Note)
3 | Key
4 | Front oil seal (See Front Oil Seal Removal Note) (See Front Oil Seal Installation Note)

## Timing Belt Pulley Lock Bolt Removal/Installation Note

1. Hold the timing belt pulley using the SSTs.

## Timing Belt Pulley Removal Note

1. Remove the timing belt pulley using the SST.

## Front Oil Seal Removal Note

1. Cut the oil seal lip using a razor knife.

2. Remove the oil seal using a screwdriver protected with a rag.

## Front Oil Seal Installation Note

1. Apply clean engine oil to the oil seal lip.

2. Push the oil seal slightly in by hand.

3. Tap the oil seal in evenly using the SST and a hammer. The oil seal must be tapped in until it is flush with the edge of the oil pump body.

Pushing distance of the front oil seal (from the edge of the oil pump body)

  0-0.5 mm {0-0.019 in}