#
INTAKE SHUTTER VALVE POSITION SENSOR CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1223800
• Consists of an integrated intake shutter valve position sensor and intake shutter valve.
• Installed to the valve shaft so that it is linked to the opening and closing of the intake shutter valve.

1 | Intake shutter valve position sensor
2 | Intake shutter valve body
3 | Shutter valve
4 | Shutter valve shaft

• Hall element sensor has been adopted for the detecting element. With the adoption of a non-contact type sensor, durability is improved.

1 | Intake shutter valve position sensor
2 | Hall element
3 | Magnet
4 | Intake shutter valve position sensor output voltage characteristic
5 | Shutter valve closing angle
6 | Output voltage
7 | High
8 | Low
9 | Open
10 | Closed