#
INSPECTION OF SST (DEPLOYMENT TOOL)

id081000801000

1. Before using the SST (49 H066 002), inspect its operation.

## Inspection Procedure

1. Follow the steps below to inspect the SST (49 H066 002).

  • If not as indicated in the table, replace the SST (49 H066 002) because it has a malfunction.

  Warning

  • Do not use a malfunctioning SST (49 H066 002), otherwise it could cause the air bag module or pre-tensioner front buckle to accidentally operate (deploy).

  Caution

  • Because the permissible voltage for the SST (49 H066 002) is 12 V, do not connect a 24 V power source because it will damage the SST. Always connect only a 12 V power source.

Step | Inspection procedure | Light condition
--- | --- | ---
Green | Red
1 | Connect the power supply red clip to the positive battery terminal, and the black clip to the negative battery terminal. | On | Off
2 | Connect connectors A and B. | Off | On
3 | Press the activation switch. | On | Off