#
PID/DATA MONITOR TABLE [MULTIPLEX COMMUNICATION SYSTEM]

id0902e6862100

PID name (definition) | Condition | Specification | PID monitor module | Terminal
--- | --- | --- | --- | ---
ABS_MSG (Missing message from the ABS HU/CM or DSC HU/CM | Present | Circuit in the ABS HU/CM or DSC HU/CM is normal | Instrument cluster | • ABS (ABS/TCS) HU/CM: O, R • DSC HU/CM: AF, AG • Instrument cluster: 2W, 2X
Not Present | Circuit in the ABS HU/CM or DSC HU/CM is abnormal
TCM_MSG (Missing message from the TCM) | Present | Circuit in the TCM is normal | • ABS/TCS HU/CM • Instrument cluster
Not Present | Circuit in the TCM is abnormal
AWD_MSG (Missing message from the 4WD control module) | Present | Circuit in the 4WD control module is normal | • DSC HU/CM • Instrument cluster
Not Present | Circuit in the 4WD control module is abnormal
IC_MSG (Missing message from the instrument cluster) | Present | Circuit in the instrument cluster is normal | DSC HU/CM
Not Present | Circuit in the instrument cluster is abnormal
PCM_MSG (Missing message from the PCM) | Present | Circuit in the PCM is normal | • ABS (ABS/TCS) HU/CM • DSC HU/CM • Instrument cluster
Not Present | Circuit in the PCM is abnormal
RKE_MSG (Missing message from the keyless control module) | Present | Circuit in the keyless control module is normal | Instrument cluster
Not Present | Circuit in the keyless control module is abnormal