#
INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [FS5A-EL]

id051721801300

1. Disconnect the negative battery cable.

2. Remove the battery and battery tray.

3. Remove the air cleaner component. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

4. Disconnect the input/turbine speed sensor connector.

5. Remove the input/turbine speed sensor.

6. Apply ATF to a new O-ring and install it on a new input/turbine speed sensor.

7. Install the input/turbine speed sensor.

Tightening torque

  8-11 N·m {82-112 kgf·cm, 71-97 in·lbf}

8. Connect the input/turbine speed sensor connector.

9. Install the air cleaner component. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

10. Install the battery and battery tray.

11. Connect the negative battery cable.