#
PRECAUTION (SUSPENSION)

id021000800100

## Wheels and Tires Removal/Installation

1. When a wheel is installed, tighten it to

88-118 N·m {9.0-12.0 kgf·m, 65.0-87.0 ft·lbf}.

## Suspension Links Removal/Installation

1. Tighten any part of the suspension that uses rubber bushings only after the vehicle has been lowered and unloaded.

Note

  • Unloaded: Fuel tank is full. Engine coolant and engine oil are at specified levels. Spare tire, jack and tools are in designated position.

## Brake Lines Disconnection/Connection

  Caution

  • Brake fluid will damage painted surfaces. If brake fluid does get on a painted surface, wipe it off immediately.

1. Tighten the brake pipe flare nut using the SST (49 0259 770B). Be sure to modify the brake pipe flare nut tightening torque to allow for use of a torque wrench-SST combination.

(See SERVICE CAUTIONS.)

2. If any brake line has been disconnected anytime during the procedure, add brake fluid, bleed the brakes, and inspect for leakage after the procedure has been completed.

## Power Steering Components Removal/Installation

1. If any power steering fluid line has been disconnected anytime during the procedure, add ATF M-III or equivalent (e.g. Dexron®II), bleed the fluid line, and inspect for leakage after the procedure has been completed.