KOEO/KOER SELF-TEST [MZR-CD (RF Turbo)]

id0102f1100400

KOEO/KOER self-test function table

×: Applicable –: Not applicable

DTC | Condition | KOEO | KOER
--- | --- | --- | ---
P0016 | CKP-CMP correlation | — | —
P0030 | A/F sensor heater control circuit problem | — | —
P0045 | Variable boost control (VBC) solenoid valve control circuit low or high input | — | ×
P0071 | Exhaust gas pressure correction temperature sensor circuit range/performance malfunction | — | —
P0072 | Pressure correction temperature sensor circuit low input | × | ×
P0073 | Pressure correction temperature sensor circuit high input | × | ×
P0088 | Fuel pressure system too high | — | ×
P0089 | Fuel pressure regulator performance | — | ×
P0093 | Fuel system leak detection | — | ×
P0096 | Intake air temperature (IAT) sensor No.2 circuit range/performance malfunction | — | —
P0097 | Intake air temperature (IAT) sensor No.2 circuit low input | × | ×
P0098 | Intake air temperature (IAT) sensor No.2 circuit high input | × | ×
P0101 | Mass airflow (MAF) sensor range/performance malfunction | — | —
P0102 | Mass airflow (MAF) sensor circuit low input | × | ×
P0103 | Mass airflow (MAF) sensor circuit high input | × | ×
P0104 | Mass airflow (MAF) sensor circuit malfunction | — | —
P0106 | Boost sensor range/performance malfunction | — | —
P0107 | Boost sensor circuit low input | × | ×
P0108 | Boost sensor circuit high input | × | ×
P0111 | Intake air temperature (IAT) sensor No.1 range/performance malfunction | — | —
P0112 | Intake air temperature (IAT) sensor No.1 circuit low input | × | ×
P0113 | Intake air temperature (IAT) sensor No.1 circuit high input | × | ×
P0116 | Engine coolant temperature (ECT) sensor range/performance malfunction | — | —
P0117 | Engine coolant temperature (ECT) sensor circuit low input | × | ×
P0118 | Engine coolant temperature (ECT) sensor circuit high input | × | ×
P0121 | Accelerator pedal position (APP) sensor No.1/No.2 position correlation | — | —
P0122 | Accelerator pedal position (APP) sensor No.1 circuit low input | × | ×
P0123 | Accelerator pedal position (APP) sensor No.1 circuit high input | × | ×
P0131 | A/F sensor circuit low input | — | —
P0132 | A/F sensor circuit high input | — | —
P0133 | A/F sensor circuit malfunction | — | —
P0134 | A/F sensor no activity detected | — | ×
P0140 | A/F sensor no activity | — | —
P0151 | A/F sensor circuit low input | — | —
P0152 | A/F sensor circuit high input | — | —
P0154 | A/F sensor circuit no activity detected | — | —
P0181 | Fuel temperature sensor circuit range/performance malfunction | — | —
P0182 | Fuel temperature sensor circuit low input | × | ×
P0183 | Fuel temperature sensor circuit high input | × | ×
P0191 | Fuel pressure sensor range/performance malfunction | — | —
P0192 | Fuel pressure sensor circuit low input | × | ×
P0193 | Fuel pressure sensor circuit high input | × | ×
P0201 | Fuel injector No.1 operation identified | — | ×
P0202 | Fuel injector No.2 operation identified | — | ×
P0203 | Fuel injector No.3 operation identified | — | ×
P0204 | Fuel injector No.4 operation identified | — | ×
P0219 | Engine overspeed condition | — | —
P0222 | Accelerator pedal position (APP) sensor No.2 circuit low input | × | ×
P0223 | Accelerator pedal position (APP) sensor No.2 circuit high input | × | ×
P0234 | Turbocharger overboost condition | — | —
P0299 | Turbocharger underboost condition | — | —
P0301 | Cylinder No.1 misfire detection | — | ×
P0302 | Cylinder No.2 misfire detection | — | ×
P0303 | Cylinder No.3 misfire detection | — | ×
P0304 | Cylinder No.4 misfire detection | — | ×
P0336 | CKP sensor range/performance malfunction | — | —
P0337 | CKP sensor circuit low input | — | —
P0341 | CMP sensor range/performance malfunction | — | —
P0342 | CMP sensor circuit low input | — | —
P0400 | EGR flow problem | — | ×
P0401 | EGR flow insufficient detected | — | —
P0402 | EGR flow excessive detected | — | —
P0403 | EGR control circuit | × | ×
P0404 | EGR control circuit range/performance | × | ×
P0405 | EGR sensor circuit low input | × | ×
P0406 | EGR valve position sensor No.1 circuit high input | × | ×
P0500 | VSS circuit malfunction | — | —
P0504 | Brake switch circuit problem | — | —
P0512 | Engine switch circuit high input | — | —
P0545 | Exhaust gas temperature sensor (upper) circuit low input | × | ×
P0546 | Exhaust gas temperature sensor (upper) circuit high input | — | ×
P0548 | Exhaust gas temperature sensor (middle) circuit low input | × | ×
P0549 | Exhaust gas temperature sensor (middle) circuit high input | — | ×
P0562 | Battery voltage low input | — | —
P0563 | Battery voltage high input | — | —
P0564 | Cruise control switch circuit malfunction | — | —
P0601 | Internal control module memory check sum error | × | ×
P0602 | PCM programming error | × | ×
P0605 | PCM memory check sum error | × | ×
P0606 | PCM malfunction | × | ×
P0607 | PCM performance problem | × | ×
P0610 | PCM vehicle options error | × | ×
P0628 | Suction control valve circuit low input | — | ×
P0629 | Suction control valve circuit high input | — | ×
P0704 | Clutch switch circuit malfunction | — | —
P0850 | Neutral switch circuit malfunction | — | —
P1196 | Key off voltage high | — | —
P1211 | Common rail pressure higher/lower than desired (engine running) | — | ×
P1281 | Common rail pressure higher than desired (engine running) | — | ×
P1303 | EGR calibration fault | — | —
P1329 | Common rail pressure higher than desired (engine running) | — | —
P1378 | Fuel injector supply voltages circuit low input | — | ×
P1379 | Fuel injector supply voltages circuit high input | — | ×
P1391 | Glow plug circuit low input | × | —
P1392 | Glow plug circuit high input | — | —
P1588 | Intake shutter valve construction problem | — | —
P1589 | Intake shutter valve control range/performance | — | ×
P1675 | Injector data not programmed | × | ×
P1676 | Checksum corrupt | × | ×
P2002 | Diesel particulate filter efficiency less than threshold | — | —
P2032 | Exhaust gas temperature sensor (lower) circuit low input | × | ×
P2033 | Exhaust gas temperature sensor (lower) circuit high input | — | ×
P2101 | Intake shutter valve position sensor circuit high input | — | ×
P2105 | Intake shutter valve actuator control system-forced engine shutdown | — | —
P2135 | Accelerator pedal position (APP) sensor No.1/No.2 voltage correlation | — | ×
P2146 | Fuel injector No.1 and No.3 operation identified | — | ×
P2147 | Fuel injector supply circuit low input | — | ×
P2148 | Fuel injector supply voltages circuit high input | — | ×
P2149 | Fuel injector No.2 and No.4 operation identified | — | ×
P2227 | BARO sensor range/performance malfunction | — | —
P2228 | BARO sensor circuit low input | × | ×
P2229 | BARO sensor circuit high input | × | ×
P242F | Diesel particulate filter restriction-soot accumulation | — | —
P2428 | Exhaust gas temperature too high | — | —
P2452 | Exhaust gas pressure sensor circuit problem | — | —
P2453 | Exhaust gas pressure sensor circuit range/performance malfunction | — | —
P2454 | Exhaust gas pressure sensor circuit low input | × | ×
P2455 | Exhaust gas pressure sensor circuit high input | × | ×
P2456 | Exhaust gas pressure sensor circuit intermittent/erratic | — | —
P2458 | Diesel particulate filter regeneration duration | — | —
P2459 | Diesel particulate filter regeneration frequency | — | —
P252F | Engine oil level too high | — | —
P253F | Engine oil deteriorated | — | —
P2621 | Intake shutter valve position sensor circuit low output | × | ×
P2622 | Intake shutter valve position sensor circuit high output | × | ×
U0166 | Communication error to water heater unit | — | —