#
DRIVE BELT CONSTRUCTION [L8, LF, L3]

id0110a1102500
• A serpentine type drive belt with a V-ribbed belt to drive the supplemental units has been adopted. This shortens the engine length and improves serviceability.
• A front drive belt auto tensioner with an embedded coil spring has been adopted to automatically maintain the optimal drive belt tension.

Drive Belt Specification.

ITEM | L8 | LF | L3
--- | --- | --- | ---
Belt length size | mm {in} | About 2,260 {88.98} (About 2,163 {85.16}) | About 2,310 {90.94}
Belt width size | mm {in} | About 20.5 {0.81}

( ) is A/C non-equipping vehicle specification.

1 | P/S oil pump pulley
2 | Drive belt
3 | Idler pulley
4 | Generator pulley
5 | Front drive belt auto tensioner
6 | Crankshaft pulley
7 | A/C compressor pulley
8 | Water pump pulley