EXHAUST GAS PRESSURE SENSOR/EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0140f1445900

  Caution
  • Because the output characteristics of the exhaust gas pressure sensor are adjusted while it is installed to the bracket, replace the exhaust gas pressure sensor and the bracket as a single unit.

  Note
  • If the exhaust gas pressure sensor is replaced, always perform each adjustment procedure using the following steps.

  STEP | ACTION | PAGE/CONDITION
  --- | --- | ---
  1 | Replace the exhaust gas pressure sensor/exhaust gas pressure correction temperature sensor. | –
  2 | Turn the engine switch on. | –
  3 | Perform exhaust gas pressure sensor data reset procedure. | (See EXHAUST GAS PRESSURE SENSOR DATA RESET [MZR-CD (RF Turbo)].)
  4 | Start the engine. | Verify that the MIL dose not illuminate.
  5 | Turn the engine switch off. | –
  6 | Turn the engine switch on (Engine off). | –
  7 | Perform KOEO self-test procedure. | (See KOEO/KOER SELF TEST [MZR-CD (RF Turbo)].)
  8 | Perform diesel particulate filter reset procedure. | (See DIESEL PARTICULATE FILTER RESET [MZR-CD (RF Turbo)].)
  9 | Turn the engine switch off. | –
  10 | Wait for 20 s. | –
  11 | Start the engine. | –
  12 | Perform diesel particulate filter assessment procedure. | Engine coolant temperature 60 °C {140 °F} or more. (See DIESEL PARTICULATE FILTER ASSESSMENT [MZR-CD (RF Turbo)].)
  13 | Turn the engine switch off. | –

1. Disconnect the negative battery cable.

2. Remove the under cover.

3. Remove in the order indicated in the table.

am6zzw00004728

1 | Exhaust gas pressure hose (See Exhaust Gas Pressure Hose Installation Note)
2 | Exhaust gas pressure sensor
3 | Exhaust gas pressure correction temperature sensor

4. Install in the reverse order of removal.

Exhaust Gas Pressure Hose Installation Note

1. Install the exhaust gas pressure hose as shown in the figure.

am6zzw00004729