#
NO.2 CD PLAYER/CHANGER DOES NOT EJECT THE CD.

id0903a1826200

2 | CD player/changer does not eject the CD./03:Er01, 06:Er01, 10:Er01, 22:Er01
TROUBLESHOOTING HINTS • Audio units is malfunctioning. • Defective CD. (e.g., cracked, badly bent, rough edges, scratch, dirty CD, condensation). • Non-conventional discs. (e.g., 8cm (3 in) CD, 8cm (3 in) disc adapter, heart-shaped disc, octagonal disc) • Poor connection of audio unit connector or terminal. (e.g., damaged, bent, pulled-out pin, corrosion) • Improper center panel installation. • Improper CD cover installation. • Deformed disc is used. (e.g., out of specification (thickness), bent disc). • Multiple CDs are inserted into the CD player at the same time.

  Note

• The CD may be malfunctioning if the CD player/changer does not eject the certain CD only. Inspect the CD player/changer operation using the CD known to be good.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Inspect the operation of the audio system other than CD player/changer (e.g. Radio). • Does other audio system operate? | Yes | Go to Step 3.
No | Go to the next step.
2 | • Turn the ignition switch to the LOCK position. • Inspect the connection of the audio unit connector (24-pin). • Inspect both audio unit connector and wiring harness-side connector for poor connection (such as damaged/bent/pulled-out pins, corrosion) • All the pins and connector normal? | Yes | Go to the next step.
No | if the audio unit connector/pin is wrong: Replace the audio unit. If the wiring harness-side connector/pin is wrong: Repair or replace the pins and/or the connector.
3 | • Eject the CD. • Is the CD ejected from the CD player/changer? | Yes | Go to the next step.
No | Inspect the center panel and CD cover installation. Securely install the center panel and/or CD cover as necessary.
4 | • Insert the CD into the CD player/changer. • Does the CD insert into the Cd player/changer smoothly? | Yes | Replace the audio unit.
No | Install the center panel and/or CD cover properly, then go to the next step.
5 | • Is the CD ejected from the CD player/changer? | Yes | Troubleshooting completed. Explain repairs to the customers.
No | Replace the audio unit.