#
LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [WGN]

id0917004631a2

1. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

2. Remove the liftgate side trim.

3. Pull the handle toward you, then remove it.

4. Pull the liftgate lower trim toward you, then disengage the clips A and pins B, C from the body.

5. Remove the liftgate lower trim.

6. Install in the reverse order of removal.