#
TORQUE CONVERTER CLUTCH (TCC) CONTROL OUTLINE [JA5AX-EL]

id051705108600

## Features

• The TCM selects the TCC schedule according to the gear selected by the transaxle. 50 Hz (20 ms cycle) on/off signals are relayed from the TCC schedule and speed sensor and throttle opening angle to the duty cycle TCC solenoid valve to control TCC.

## Construction (System Diagram)

.

1 | VSS
2 | Input/turbine speed sensor
3 | Engine speed signal
4 | Throttle position signal
5 | TCC signal
6 | PCM
7 | CAN
8 | TFT sensor
9 | TCM
10 | TR switch
11 | TCC solenoid valve
12 | R
13 | D
14 | N
15 | P