#
DOUBLE CONE SYNCHRONIZER MECHANISM CONSTRUCTION/OPERATION [G66M-R]

id0515k1100200
• The basic construction of the double cone synchronizer mechanism is the same as a triple cone synchronizer mechanism except that the inner side of the inner cone is not used as a friction surface.
• The basic construction of the double cone synchronizer mechanism is the same as a triple cone synchronizer mechanism except that friction force is not generated because there is no contact surface between the inner cone and each gear.
• For the triple cone synchronizer mechanism operation, refer to the G35M-R manual transaxle triple cone synchronizer mechanism. (See TRIPLE CONE SYNCHRONIZER MECHANISM OPERATION [G35M-R].)