CONNECTING ROD INSPECTION

id011000502800

1. Inspect the connecting rod for bending and distortion using the connecting rod aligner.

If it is at the maximum specification or more, replace the connecting rod.

amj2224e255

  Maximum connecting rod bending [per 50 mm]

  0.070 mm {0.0019 in}

  Maximum connecting rod distortion [per 50 mm]

  0.060 mm {0.0027 in}

  Connecting rod center-to-center distance

  150.65—150.75 mm {5.9311—5.9350 in}