#
A/C CUT-OFF CONTROL OPERATION [MZR-CD (RF Turbo)]

id0140f1103700
• When the accelerator opening angle is 60 % or more, the PCM cuts the power supply to the A/C relay for 5 s.
• When the engine coolant temperature is 113 °C {235 °F} or more, the PCM switches the power supply to the A/C relay every 10 s.
• When diesel particulate filter regeneration is performed using the WDS or equivalent, the power supply to the A/C relay is cut.