#
REAR DOOR LOCK ACTUATOR INSPECTION

id0914z6430700

## Door Lock Actuator

1. Disconnect the rear door lock actuator connector.

2. Apply battery positive voltage to the rear door lock actuator terminals and inspect the operation of the rear door lock actuator.

  • If not as specified, replace the rear door lock actuator.

With double locking system

Connection | Actuator operation
--- | ---
B+ | GND
A (F) | F (A) | Lock
F (A) | A (F) | Double lock
F and E (A and B) | E (A) | Unlock

  ( ) :
RH

Without double locking system

Actuator operation | Connection
--- | ---
B+ | GND
Lock | A (F) | B (E)
Unlock | B (E) | A (F)

  ( ) :
RH

## Door Lock-link Switch (With Theft-deterrent System

1. Disconnect the rear door lock actuator connector.

2. Inspect for continuity between the door lock-link switch terminals using an ohmmeter.

  • If not as specified, replace the rear door lock actuator.