#
STEERING ANGLE SENSOR INSPECTION

id091800802700

## With DSC

1. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

2. Disconnect the steering angle sensor connector.

3. Connect battery positive voltage to terminal A and ground to terminal F of the steering angle sensor.

4. Turn the steering wheel to the right and left, and verify that the voltage and pulses at the terminals are as shown in the figure.

  • If there is any malfunction, replace the body of the combination switch.