#
AUTOMATIC TRANSAXLE FEATURES

D6E051700000A05

Realization of excellent shift quality | • Electronic pressure-adjusting control of line pressure by a liner type solenoid (pressure control solenoid A) adopted • Electronic control (direct electric shift control) of clutch pressure by duty-cycle type solenoids (shift solenoid A, B, and C, pressure control solenoid B) adopted
Superior shift quality | • Centrifugal balance clutch chamber adopted
High efficiency, compactness, lightweight | • Miniature trochoid gear oil pump with torque converter direct drive adopted
Improved reliability | • Variable resistor type TR switch has been adopted
Improved marketability | • Sport AT adopted • Sub-shifting mechanism has been adopted
Improved reliability, reduced noise and vibration | • A double arranged gear with a single planetary gear unit is has been adopted as the main shifting mechanism • A single planetary gear unit is has been adopted as the sub-shifting mechanism