SIMULATION TEST [L3 Turbo]

id0102b7100600

• The simulation test items for the fuel and emission control systems are as shown in the table below.

Simulation item table

×: Applicable
—: Not applicable

Item | Applicable component | Operation | Test condition | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
ACCS | A/C relay | On/Off | × | × | 4N
ALTF | Generator field coil control | On/Off | — | × | 1AD
EVAPCP | Purge solenoid valve | % | × | × | 4T
FAN_DUTY | Fan control | % | × | × | 4A
FP | Fuel pump relay | On/Off | × | × | 4Q
FUELPW1 | Fuel injection duration | % | — | × | 3B, 3E, 3H, 3K
GENVDSD | Generator voltage desired | V | — | × | —
HTR11 | A/F sensor heater | On/Off | × | × | 4AD
HTR12 | HO2S heater | On/Off | × | × | 4Z
IMRC | Variable swirl solenoid valve | On/Off | × | × | 4K
INJ_1 | Fuel injector (Cylinder No.1) | Off | — | × | 3B
INJ_2 | Fuel injector (Cylinder No.2) | Off | — | × | 3E
INJ_3 | Fuel injector (Cylinder No.3) | Off | — | × | 3H
INJ_4 | Fuel injector (Cylinder No.4) | Off | — | × | 3K
SEGRP | EGR valve (stepping motor) | step | × | × | 4D, 4G, 4J, 4M
test | Test mode | On/Off | × | × | —
VT DUTY1 Wt | Camshaft position commanded duty cycle | % | × | × | 4S
WGC | Wastegate control solenoid valve | % | × | × | 4H