#
INSTRUMENT CLUSTER OUTLINE

id092200100200
• A CAN system has been adopted for the control signals of the input/output communication circuit of the meters, gauges and warning and indicator lights. (See CONTROLLER AREA NETWORK (CAN) SYSTEM OUTLINE.)
• LEDs have been adopted for all warning and indicator lights installed on the instrument cluster.
• The information display, which includes clock, audio system, and A/C system displays, has been placed in the center of the instrument panel. It also includes the drive information system, depending on the vehicle grade.
• A trumpet-type horn with spiral, resonant pipes, has been adopted.

## Specifications

Item | Specification
--- | ---
Speedometer | Meter type | Stepping motor type
Indication range | (km/h) | 0-240 (except L3 turbo) 0-280 (L3 turbo)
(mph {km/h}) | 0-150 {0-240} (except L3 turbo) 0-180 {0-280} (L3 turbo)
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Tachometer | Meter type | Stepping motor type
Indication range | (rpm) | 0-8,000 (L3, L3 turbo, LF, L8), 0-6,000 (MZR-CD (RF Turbo))
Red zone | (rpm) | 6,500-8,000 (L3, L3 turbo, LF, L8) 5,000-6,000 (MZR-CD (RF Turbo))
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Fuel gauge | Meter type | Stepping motor type (Reset-to-zero type)
Input signal communication system | Conventional communication system
Input signal source | Fuel tank gauge unit
Rated voltage | (V) | DC 12
Water temperature gauge | Meter type | Stepping motor type (Medium range stabilized type)
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Odometer/Tripmeter | Display | LCD
Indication digits | Odometer: 6 digits, Tripmeter: 4 digits
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Warning alarms | Sound frequency | (Hz) | 1,500-2,400
Output sound pressure level | (dB) | 67.5-85.0
Lights-on reminder warning alarm | Sound frequency | (Hz) | 1,500
Sound cycle |
Seat belt warning alarm | Sound frequency | (Hz) | 2,400
Sound cycle |
Key reminder warning alarm | Sound frequency | (Hz) | 1,500
Sound cycle |
Advanced keyless entry system warning alarm | Sound frequency | (Hz) | 1,500
Sound cycle |
Indicator alarm | Output sound pressure level | (dB) | 55.0
Turn and hazard indicator alarm | Sound cycle |