#
DLC-2 CONSTRUCTION

id040200100600
• The data link connector-2 (DLC-2) is composed of 16-pin connectors containing terminals KLN, CAN_H, CAN_L, +B, GND1, and GND2.

Terminal | Function | Remark
--- | --- | ---
KLN | • Outputs DTC related to ABS (ABS/TCS) or DSC HU/CM • PID/DATA monitor and record function • Active command modes function | WDS or equivalent communication line
CAN_H | CAN line (HI) | - | -
CAN_L | CAN line (LO) | - | -
GND1 | Body ground | - | -
GND2 | Ground for WDS or equivalent | - | -
B+ | Battery positive voltage for WDS or equivalent | - | -