#
PRIMARY SHAFT COMPONENTS INSPECTION

D6E051517040102

## Primary Shaft and Gear Inspection

1. Inspect the shaft for damage, abnormal wear, dents, flaking, or bending.

  • If there is any malfunction, replace the shaft.

2. Inspect the gears for damage, abnormal wear, dents, flaking, or bending.

  • If there is any malfunction, replace the gear.

## Bearing Inspection

1. Verify that the bearing to rotates smoothly.

  • If there is any malfunction, replace the bearing.