#
NO.24 ENGINE STALLS WHEN SHIFTED TO D, M RANGES, OR IN R POSITION [FS5A-EL]

id050308808700

24 | Engine stalls when shifted to D, M ranges, or in R position
DESCRIPTION | • Engine stalls when shifting from N or P position to D, M ranges or R position at idle.
POSSIBLE CAUSE | • The malfunction is on the engine control side (i.e. electronic throttle control system). Otherwise, the malfunction is in the input/turbine speed sensor (engine sometimes starts) or the TCC circuit (engine always stalls).

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Go to symptom troubleshooting No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [L8, LF, L3].) Is the engine control system normal? | Yes | Repeat the basic inspection and repair or replace any malfunctioning parts according to the inspection result. (See BASIC INSPECTION [FS5A-EL].)
No | Repair or replace any malfunctioning parts according to the inspection results.
2 | • Verify the test results. - If normal, return to the diagnostic index to service any additional symptoms. - If the malfunction remains, inspect the related Service information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting is completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.