#
DTC P0610 [MZR-CD (RF Turbo)]

id0102f1809600

DTC P0610 | PCM vehicle options error
--- | ---
DETECTION CONDITION | • PCM data configuration error
POSSIBLE CAUSE | • Configuration procedure has not been completed • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY TROUBLESHOOTING OF DTC P0610 COMPLETED • Make sure to reconnect all disconnected connectors. • Turn the engine switch to the ON position (Engine off). • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Are any DTC present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.