#
VEHICLE SPEED SENSOR INSPECTION (WITHOUT ABS) [G66M-R]

id0515k1801100

1. Remove the vehicle speed sensor.

(See VEHICLE SPEED SENSOR REMOVAL/INSTALLATION (WITHOUT ABS) [G66M-R].)

2. Measure the voltage between the vehicle speed sensor terminals while the gear is turning.

Meter needle | Action
--- | ---
Moves slightly under 5 V (AC) | Inspect wiring harness between instrument cluster and vehicle speedometer sensor.
Does not move | Replace vehicle speed sensor.

3. Install the vehicle speed sensor.

(See VEHICLE SPEED SENSOR REMOVAL/INSTALLATION (WITHOUT ABS) [G66M-R].)