#
CLUTCH HOUSING AND TRANSAXLE CASE COMPONENTS ASSEMBLY [TYPE A]

id051500803812

1. Assemble in the order indicated in the table.

1 | Oil passage
2 | Oil seal (differential) (See Oil Seal (Differential) Assembly Note.)
3 | Adjustment shim
4 | Bearing race (differential) (See Bearing Race (Differential) Assembly Note.)
5 | Adjustment shim
6 | Bearing race (transaxle case) (See Bearing Race (Transaxle Case) Assembly Note.)
7 | Drain plug and washer
8 | Inner shift lever
9 | Push pin component and spring
10 | Bearing race (differential) (See Bearing Race (Differential) Assembly Note.)
11 | Oil seal (differential) (See Oil Seal (Differential) Assembly Note.)
12 | Hole cover
13 | Breather
14 | Breather cover component
15 | Control rod
16 | Selector
17 | Roll pin
18 | Change arm
19 | Roll pin
20 | Sealing cap
21 | Guide plate
22 | Funnel
23 | Bearing race (secondary shaft)
24 | Oil seal (primary shaft) (See Oil Seal (Primary Shaft) Assembly Note.)
25 | Bearing race (primary shaft)
26 | Boots
27 | Spring and washer
28 | Key
29 | Control end
30 | Shift lever shaft
31 | Shift lever component
32 | Roll pin

## Oil Seal (Differential) Assembly Note

1. Apply transaxle oil to the new oil seal lip.

2. Install the oil seal using the SST.

## Bearing Race (Differential) Assembly Note

1. Install the adjustment shim(s) and install the bearing race using the SST.

## Bearing Race (Transaxle Case) Assembly Note

1. Install the adjustment shim(s) and install the bearing race using the SST.

Primary shaft side

Secondary shaft side

## Oil Seal (Primary Shaft) Assembly Note

1. Apply transaxle oil to outer circumference of the oil seal.

2. Install the new oil seal using the SST.