#
DTC P0706 [FS5A-EL]

id050221800900

DTC P0706 | Transaxle range (TR) switch range/performance
--- | ---
DETECTION CONDITION | • When all conditions below are satisfied and 100 s or more have passed. - Engine speed 530 rpm or more - Vehicle speed 20 km/h {12 mph} or more - Voltage at TCM terminal 2H 0.5 V or more - P, R, N, or D range/position not detected Diagnostic support note: • This is a continuous monitor (CCM). • The MIL illuminates if the TCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the TCM. • The PENDING CODE is available if the TCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA is available. • The AT warning light illuminates. • The DTC is stored in the TCM memory.
POSSIBLE CAUSE | • TR switch malfunction • TR switch misadjustment • TCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has the FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT TR SWITCH • Turn the ignition switch to the LOCK position. • Disconnect the TR switch connector. • Inspect for resistance between TR switch terminals B and C (part-side). • Is the resistance normal? (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FS5A-EL].) | Yes | Adjust the TR switch, then go to the next step. (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [FS5A-EL].)
No | Replace the TR switch, then go to the next step. (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [FS5A-EL].)
4 | VERIFY TROUBLESHOOTING OF DTC P0706 COMPLETED • Make sure to reconnect all the disconnected connectors. • Clear the DTC from the memory using the WDS or equivalent. • Drive the vehicle in each range (D and R) for 100 s or more under the following conditions: - Engine speed (RPM PID): 530 rpm or more - Vehicle speed (VSS PID): 20 km/h {12 mph} or more • Is the PENDING CODE present? | Yes | Replace the TCM, then go to the next step. (See TCM REMOVAL/INSTALLATION [FS5A-EL].)
No | No concern is detected. Go to the next step.
5 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [FS5A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection.
No | DTC troubleshooting completed.