#
TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5AX-EL]

id051705800900

  Note

  • Input signals of the TR switch can be inspected with a WDS or equivalent. (See TCM INSPECTION [JA5AX-EL].)

## Inspection of Operation

1. Verify that the starter operates only with the ignition switch at the START position and the selector lever in P and N positions.

  • If not as specified, inspect for continuity at the TR switch. (See Inspection of Continuity.)

2. Verify that the back-up lights illuminate when shifted to R position with the ignition switch at the ON position.

  • If not as specified, inspect for continuity at the TR switch.

## Inspection of Continuity

1. Disconnect the TR switch connector.

2. Inspect for continuity at the TR switch.

  • If not as specified, adjust the TR switch, then reinspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [JA5AX-EL].)

3. Connect the TR switch connector.