#
FOREWORD [AUDIO]

id0903a18226e4
• Refer to section 00 and thoroughly read and understand the basic flow of troubleshooting in order to properly perform the procedures.
• For the steps that have an asterisk (*), inspect the connector/terminal connection for continuity and damage. If the connection is poor, reconnect it, or repair or replace the appropriate parts if necessary.

## TROUBLESHOOTING INDEX

CASSETTE TAPE PLAYER
NO. | Symptom | Possible DTC
--- | --- | ---
1 | No sound of the cassette tape. | 00:Er01, 00:Er03, 00:Er10
2 | Cassette tape player does not eject the cassette tape. | 00:Er01, 00:Er04, 00:Er10
3 | Cassette tape player does not load the cassette tape. | 00:Er01, 00:Er10
4 | Cassette tape player ejects the cassette tape immediately. | 00:Er04, 00:Er10
5 | Wavering sound and/or poor sound quality of the cassette tape. | -
6 | There is a noise when playing the cassette tape player. | -
7 | Poor sound qualoty.(Poor treble sound) | -
8 | Abnormal sound of the cassette tape. (Play backwards) | -