#
SECONDARY SHAFT (NO.1) COMPONENTS PREINSPECTION

D6E051517040104

## Thrust Clearance Inspection

1. Measure the thrust clearance of each gear using a feeler gauge and a dial gauge.

  Secondary shaft (NO.1) gear thrust clearance
(mm {in})

Gear | Thrust clearance
--- | ---
1st | 0.10-0.35 {0.0039-0.0138}
2nd | 0.11-0.46 {0.0044-0.0181}
3rd | 0.11-0.54 {0.0044-0.0212}
4th | 0.10-0.65 {0.0039-0.0255}

  • If not within the specification, replace the malfunctioning parts.

## Radial Clearance Inspection

1. Measure the radial clearance of each gear using a dial gauge.

  Secondary shaft (NO.1) gear radial clearance
(mm {in})

Gear | Radial clearance
--- | ---
1st | 0.015-0.068 {0.00059-0.00267}
2nd | 0.015-0.048 {0.00059-0.00188}
3rd | 0.015-0.066 {0.00059-0.00259}
4th | 0.015-0.066 {0.00059-0.00259}

  • If not within the specification, replace the malfunctioning parts.