#
TRANSFER OIL REPLACEMENT [A26MX-R]

id0316d3800300

1. Remove the drain plug with the washer.

2. Drain the oil into a suitable container.

3. Tighten the drain plug with a new washer.

Tightening torque

  39.2-58.8 N·m {4.0-5.9 kgf·m, 29.0-43.3 ft·lbf}

4. Remove the oil level plug with the washer and add the specified amount and type of oil through the oil level plug hole until the level reaches the bottom of the oil level plug hole.

Transfer oil [A26MX-R]

  Specified oil grade: API Service GL-5
  Specified oil viscosity: SAE 80W- 90
  Capacity (approximate quantity): 1.2 L {1.3 US qt, 1.1 lmp qt}

5. Tighten the oil level plug with a new washer.

Tightening torque

  39.2-58.8 N·m {4.0-5.9 kgf·m, 29.0-43.3 ft·lbf}