#
FRONT BUMPER REMOVAL/INSTALLATION

id091000405100

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Screw A
2 | Fastener A
3 | Screw B
4 | Bolt
5 | Fastener B
6 | Front bumper (See Front Bumper Removal Note) (See Front Bumper Installation Note)

3. Install in the reverse order of removal.

## Front Bumper Removal Note

1. Pull the front bumper ends (wheel arch) outward to disengage from the bumper slider.

  Caution

  • If only one side of the front bumper is disengaged from the bumper slider and the bumper falls, it could be damaged. When disengaging the front bumper from the slider, secure the bumper so that it does not fall.

2. Remove the front bumper from the body.

## Front Bumper Installation Note

1. Spread the front bumper ends (wheel arches) apart.

2. Attach the front bumper to the body.

3. Press the front bumper connection portion into the body to engage with the bumper slider.