#
POWER DOOR LOCK SYSTEM OPERATION [ADVANCED KEYLESS SYSTEM]

id0914b51010b1
• When the driver's door is locked/unlocked with the driver's door lock knob or key cylinder, the door lock-link switch in the door lock actuator is locked/unlocked via the rod.
• The BCM (body control module) activates each lock actuator to lock/unlock according to the lock/unlock signal from the door lock-link switch.

1 | Driver's door lock knob
2 | Driver's door key cylinder
3 | Door lock-link switch (in driver's door lock actuator)
4 | BCM
5 | Lock Actuator