#
DTC C1508 [ABS (ABS/TCS)]

id040214874400

DTC | C1508 | TCS control
DETECTION CONDITION | • TCS control continues operation for 60 seconds or more.
POSSIBLE CAUSE | • System is normal. For protection of solenoid valves in the ABS (ABS/TCS) HU/CM, or protection of the engine, sustained and continual control of TCS is inhibited.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear the DTC from the memory. (See Clearing DTCs Procedures) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above. • Is same DTC present? | Yes | Replace ABS (ABS/TCS) HU/CM, then go to the next step.
No | Inspect intermittent concern using the same procedure as engine control system.
2 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | Troubleshooting completed.