#
EXTERIOR OPEN/CLOSE FUNCTION OUTLINE

id091200102000
• A exterior open/close function has been adopted so that the power window system can be operated from outside the vehicle.
• This function can operate in conjunction with the following:

  - Transmitter
  - Driver-side request switch (with advanced keyless system, close operation only)

• An auto reverse pinch protection function operates if the door glass is obstructed during close operation.

Operation item | Open operation (Automatic open) | Close operation (Manual close)
--- | --- | ---
Transmitter | UNLOCK button operation (long press, approx. 1.5 s or more) | LOCK button operation (long press, approx. 1.5 s or more)
Request switch (With advanced keyless system) | - | Long press, approx. 1.5 s or more